{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":8,"rows_kept":14,"merged":[[0,0,0,7],[6,0,6,5],[6,6,6,7]],"flags":["formulas_cached_only"]}
["安庆师范学院物资设备采购报价表 （AQSY201511-12X）"]
["序号","名  称","规格及性能指标","数量","单位","投标产品品牌、型号及规格","单价（元）","总价（元）"]
[1,"量热器","外筒尺寸为φ99×15Omm，内筒尺寸为φ68×84mm。内筒及搅拌器由铜制成，其比热容C=O.092卡/克℃。外筒表面镀铬。内外筒之间有绝缘垫圈隔开。绝缘盖用塑料做成，中间有孔用以插温度计，总重量约lKg。\n",6,"只"]
[2,"蒸汽发生器"," 用做热学实验仪器的加热汽源。特点：（带电炉）需外加热。",12,"只"]
[3,"攸英装置(弯曲杨氏模量测定仪)","  仪器利用弹性梁的弯曲，测定金属材料的杨氏模量。仪器由在基座上相对移动的两个平行刀口及搁在上面的弹性钢梁组成，钢梁中段套着具有刀口向下的矩形杠，它的下端，可悬挂砝码，当悬重P作用于钢梁而使梁弯曲时，其弛重量可通过上面安排的砝码显示表准确读取。从而计算出钢梁材料的杨氏模量。",6,"台"]
[4,"杨氏模量测定仪（拉伸法)","望远镜放大倍数:30倍 物镜有效孔径42㎜ 视场角1°26′、砝码7个、光杠杆：φ40㎜带配重锤、含水平仪测量架高1.2米.",6,"台"]
["合计（大写）： ",{"$nulls":5},"（￥         元 ）"]
["供货要求：",null,"1.合同签订之日起15个工作日内供货安装调试完毕；"]
[null,null,"2.由供货单位免费送至学校制定地点并安装调试到位，并提供三包。"]
[null,null,"3.承诺免费质保     年(至少1年）。"]
[null,null,"投标单位（公章）："]
[null,null,"联系人："]
[null,null,"手机号："]
[null,null,"日期："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}