{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":11,"n_cols":8,"rows_kept":11,"merged":[[0,0,0,7],[3,0,3,5],[3,6,3,7]],"flags":["formulas_cached_only"]}
["安庆师范学院物资设备采购报价表 （AQSY201511-13X）"]
["序号","名  称","规格及性能指标","数量","单位","投标产品品牌、型号及规格","单价（元）","总价（元）"]
[1,"信号与系统实验箱","\n一、技术性能\n1.实验箱主机规格约为：445mm×335mm×180mm；2.交直流电源,输入：AC 220V±10%,输出：DC ±15V/1A，±5V/1A，每路均有短路保护自动恢复功能;3.非正弦多波形信号发生器;输出波形：半波、全波、方波、矩形波、三角波;4.阶跃信号发生器,输出幅度0～±5V可调正阶跃、负阶跃信号;5.函数信号发生器,输出波形：正弦波、三角波、方波,输出频率范围：2Hz～2MHz分档连续可调,输出幅度：0～15VP-P连续可调，带有20dB和40dB衰减输出;6.六位数显频率计,测频范围：1Hz～10MHz，可显示信号源的输出频率以及外测输入信号的频率;7.真有效值交流数字毫伏表,测量范围：0～20V，分200mV、2V、20V三档，直键开关切换，三位半数显,频带范围：10Hz～1MHz,测量精度：±0.5%±2个字;8.信号的分解与合成模块,ADC：Linear公司的LTC1605，16bit，采样率100kbps，输入电压范围±10V,DAC：亚德诺公司的AD5348，12bit，含有8个并行DAC,FPGA：Altera公司的EP3C25E144，25000个LEs，594kb片内存储器（66个M9K存储器模块），66个18bit×18bit乘法器，4个PLL。\n二、系统组成\n（一）主板\n1.±5V、±15V直流电源;2.非正弦多波形信号发生器;3.阶跃信号发生器;4.函数信号发生器（低频）;5.六位数显频率计;6.真有效值交流数字毫伏表。\n（二）实验模块及模块配置表\n信号与系统基础实验,一阶系统的阶跃响应/二阶系统的时域响应,切比雪夫低通滤波器,无源与有源滤波器(LPF、HPF、BPF、BEF各四种),基本运算单元信号的采样与恢复,信号分解与合成模块。\n三、满足实验内容\n1.常用信号的观察;2.零输入、零状态及完全响应;3.信号的无失真传输;4.系统的能控性与能观性分析;5.一阶系统的阶跃响应;6.二阶系统的时域响应;7.基本运算单元;8.信号的采样与恢复;9.非正弦周期信号的分解与合成。",30,"台"]
["合计（大写）： ",{"$nulls":5},"（￥         元 ）"]
["供货要求：",null,"1.合同签订之日起15个工作日内供货安装调试完毕；"]
[null,null,"2.由供货单位免费送至学校制定地点并安装调试到位，并提供三包。"]
[null,null,"3.承诺免费质保     年(至少1年）。"]
[null,null,"投标单位（公章）："]
[null,null,"联系人："]
[null,null,"手机号："]
[null,null,"日期："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}