{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":8,"rows_kept":14,"merged":[[0,0,0,7],[7,0,7,3],[7,4,7,7],[8,0,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7]],"flags":["formulas_cached_only"]}
["安庆师范学院维修装饰工程采购报价表(AQSY201511-04X)"]
["序号","品目名称","产品规格及参数","投标产品品牌、型号及规格","数量","单价（元）","总价（元）","备注"]
[1,"墙面出新","改性丙烯酸外墙乳胶漆，达到国家执行标准一等品的一款外墙面漆，各项性能均达到国家一等品标准；具有较好的耐水、耐碱性能和耐擦洗性。",null,"104平米",null,null,"含工程费用和垃圾清扫，搬出校园，总价按实际面积计算。"]
[2,"吊顶天花","表面工艺: 抗油污滚涂板；尺寸: 300*300材质: 铝合金颜色分类: 钢琴烤漆款 铂金锦绣 ；含轻钢龙骨边角线等安装配件。",null,"141平米",null,null,"含工程费用和垃圾清扫，搬出校园，总价按实际面积计算。"]
[3,"投影吊架和幕布","120寸电动幕布，幕布材质：波珠。使用高亮度、增益大于2.4倍、有效散射角大于32度的幕面材料。幕表面物理参数稳定衰减小，幕面材料无任何气味，平整度好。外壳由金属板冲压机械加工成型，表面静电喷涂装饰。具有UL认证，CE认证。包安装。",null,1,null,null,"包安装"]
[4,"LED格栅灯","LED600*600，方形格栅日光灯",null,30,null,null,"含工程费用"]
[5,"防静电地板","规格：满足国际标准：FS1250，或国家标准HDM（Z）级。尺寸600*600*40mm；集中载荷：LB>=1250，N>=5563，KG>=568，冲击载荷>=670N，极限载荷>=16680N，均匀载荷>=33000N/M2，滚动载荷>=5560N/10次，滚动载荷>=4450N/10000次；防火性能：阻燃CLASS1；系统电阻1*106-1*1010欧姆；地板底面采用ST14拉伸板，表面选用SPCC硬质钢材，地板表面经过导电环氧树脂静电喷塑处理，内腔发泡水泥填充，四角冲角锁孔。支座采用镀锌LB>=1250或铸铝模压成型，丝杆可任意调节，地板四周成型有切边与焊接两种。四角支撑，支架高度可调节，组织灵活，布线力量，互换性好，维护方便。",null,"141平米",null,null,"含工程费用和废旧地板等搬出校园，总价按实际面积计算。包安装。"]
["合计：（大写）",{"$nulls":3},"（￥             元）"]
["备注：1.施工方须提供相关材料并将按时保质完成以上工程，提供三包，免费质保期    年（至少1年）。"]
[null,"2.施工方自行负责自身的施工安全并确保学校师生及财务安全，不得扰乱校园教学秩序，保证按相关法律法规要求及时清除建筑垃圾。"]
[null,"3.投标报价前须现场勘查，上表备注列所说的“实际面积”即各投标人根据现场勘查情况自行测量的面积，施工后不得增加面积和工程量，现场勘查联系人丁老师，联系电话：13955628657."]
[null,"4.工程竣工后须接受审计，审计价低于中标价，以审计价为准，审计价高于中标价，以中标价为准。"]
[null,"报价单位（公章）：",null,"联系人："]
[null,"报价日期：",null,"联系电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}