{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[14,0,14,4],[14,5,14,6]],"flags":["formulas_cached_only"]}
["安庆师范学院物资设备采购报价表 （AQSY201511-06X）"]
["序号","名  称","规格及性能指标","数量","投标产品品牌、型号及规格","单价（元）","总价（元）"]
[1,"指纹加刷ID卡门禁","1、2.4寸彩屏显示 TCP/IP和RS485通讯可选\n2、自带门铃大按键 U盘功能可上传下载记录等\n3、既可外接读头也可做为门禁读头使用\n4、指纹容量1500记录容量：50000背光数字夜间操作",2]
[2,"双门磁力锁","1、双联280KG磁力，三年质保工作电压:12VDC\n2、符合公安消防要求,断电即开锁断电后,无剩磁                                                                  3、耗电量低防腐蚀,锁体经地特殊防锈处理 ",2]
[3,"U型磁力锁支架","无框玻璃门使用",4]
[4,"后备电源\n控制箱\n","1、电压检测、充（放）电保护\n2、220V输入.12V输出.50W功率\n3、设开门按钮输入,可直接开启电锁.\n4、选配UPS电源,停电自动供电,电池电压过低自动断电,保护电池.",2]
[5,"开门按钮","门禁专用按钮",2]
[6,"配套发卡器","1、可发行IC、通讯接口：USB\n2、通讯波特率：4800b/s\n3、读卡距离：3-4cm\n4、外观尺寸：97mm*124mm*32mm",2]
[7,"遥控开门器","1、遥控开门、简单实用(1-1)\n2、体积小巧,安装简易 可一拖多个遥控器",2]
[8,"无线门铃","1、喷砂工艺装饰，包含可切换的多种铃声（30种以上）\n2、60米接收   3、铃声音质清脆，无杂音  4、开关灵敏",2]
[9,"感应卡","1、短距离感应卡，长度小于9厘米",100]
[10,"门禁系统考勤软件","1、集成门禁和考勤系统\n2、包含安装及后期维护和使用培训",1]
[11,"施工费用","包含各种设备安装及强电、弱电的安装；含一年上门维修费用",2]
[12,"线材","包含强电、弱电线材，及安装中各相关配件",2]
["合计（大写）： ",{"$nulls":4},"（￥         元 ）"]
["供货要求：",null,"1.合同签订之日起15个工作日内供货安装调试完毕；"]
[null,null,"2.由供货单位免费送至学校制定地点并安装调试到位，并提供三包。"]
[null,null,"3.承诺免费质保     年(至少1年）。"]
[null,null,"投标单位（公章）："]
[null,null,"联系人："]
[null,null,"手机号："]
[null,null,"日期："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}