{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":7,"rows_kept":7,"merged":[[0,0,0,6],[3,0,3,3],[3,4,3,6]],"flags":["formulas_cached_only"]}
["安庆师范学院仪器设备采购报价表(AQSY201210-07L)"]
["序号","仪器名称","产品规格及参数","投标产品品牌、型号及规格","数量","单价（元）","总价（元）"]
[1,"机架式服务器","2U标准机架式服务器，含相应安装支架、滑轨和kvm连接线；CPU：英特尔®至强® E5-4600系列处理器2颗，核心数可以为4、6、8，支持处理器插槽数4个。新一代高性能 DDR-3 内存，内存:8GB；RAID卡：支持RAID 0、1、5、6等，cache≥512M；PCI插槽：≥6个，至少4个以上的USB2.0接口，正面不少于1个USB接口；热插拔冗余电源；多个千兆以太网卡；支持6个及以上热插拔SAS、SATA硬盘驱动器；硬盘数量3块*2T，SAS硬盘，硬盘转速15000RPM。",null,1]
["合计：（大写）",{"$nulls":3},"（￥              元）"]
["备注：供货商负责将以上设备免费送至采购方指定地点并安装调试到位，并提供免费三包。"]
[null,"报价单位（公章）：",null,null,"联系人："]
[null,"报价日期：",null,null,"联系电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}