{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":7,"rows_kept":6,"merged":[[0,0,0,6],[3,0,3,2],[3,4,3,6]],"flags":["formulas_cached_only"]}
["安庆师范学院仪器设备采购报价表(AQSY201208-01L)"]
["序号","名  称","规格及性能指标","投标产品品牌、型号及规格","数量","单价（元）","总价（元）"]
[1,"立式空调","冷暖型,定频,3匹,使用面积：32-50平方米，能效等级:2级，制冷功率2155W，制冷量：7300W，室内机尺寸500*1720*300mm.国产名牌或合资名牌。含原厂原装相关配件及安装辅材，并免费送货、安装、调试到位。",null,16]
["合计（元）：人民币",{"$nulls":3},"（￥                ）"]
[null,"报价单位（公章）：",null,null,"联系人："]
[null,"报价日期：",null,null,"联系电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}