{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"merged":[[0,0,0,6],[9,0,9,3],[9,4,9,6],[10,0,10,6]],"flags":["formulas_cached_only"]}
["安庆师范学院仪器设备采购报价表(AQSY201504-03X)"]
["序号","品目名称","产品规格及参数","投标产品品牌、型号及规格","数量","单价（元）","总价（元）"]
[1,"汽车停车位","0.15米宽白色热融反光漆(2.5米*5米)",null,"600个"]
[2,"自行车停车位","0.15米宽白色热融反光漆",null,"8000米"]
[3,"主干道分道线","0.15米宽、2米长黄色热融反光漆",null,"8000米"]
[4,"限速标志牌","牌：Φ80，杆：长3米Φ89热镀（支架混凝土安装）",null,"10块"]
[5,"禁鸣标志牌","牌：Φ80，杆：长3米Φ89热镀（支架混凝土安装）",null,"8块"]
[6,"禁停标志牌","牌：Φ80，杆：长3米Φ89热镀（支架混凝土安装）",null,"10块"]
[7,"停车标志牌","牌：Φ80，杆：长3米Φ89热镀（支架混凝土安装）",null,"10块"]
["合计：（大写）",{"$nulls":3},"（￥        元）"]
["备注：1.供货商负责将以上设备免费送至采购方指定地点并安装调试到位，免费提供现场培训，免费三包。2.合同签订之日起10日内(含节假日）停车位、标线划设完毕，15日内(含节假日）交通标志牌安装到位。"]
[null,"报价单位（公章）：",null,"联系人："]
[null,"报价日期：",null,"联系电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}